| Login to enhance your online experience. Login or Create an Account
Categories USB 2.0 XPRS Power Supplies Enclosures Cables Software Main Menu About Us Knowledge-Base FAQS Blog Installation Software Technical-Support News Mail-List Store-Policies License-Agreement Terms-Of -Use Privacy-Statement Online Store Menu Store Home Shopping Cart Checkout Advanced Search Shopping Cart There are no items in your shopping cart. | # Email a Friend Menu: Store Home | Advanced Search | Shopping Cart | Checkout
usb2isa-r - USB 2.0 to ISA card ROHS [Click on images to enlarge] If you need to use your ISA card, but your new computer or laptop lacks ISA slots, use our usb2isa card to convert your USB port to a virtual ISA slot. Dimensions: 6 X 1.80 X 0.5 in., 15.0 X 4.5 X 1.5 cm. ROHS compliant - Yes, recommended for customers in the European Union, and all other countries. ARS Technologies’ USB2ISA® allows plugging and handling of any standard or custom ISA card. Our usb2isa provides simple migration from ISA form factor to USB, full access to memory and I/O space of the ISA card, and handling of IRQ and DMA events. The usb2isa functions on these Operating Systems: Windows - XP, Server 2003, Vista, Server 2008, 7, 8.1, 10 Linux - 3.x.xx and later kernels, x86 (32/64bit) and ARM processors (raspberry pi) Mac OS X 10.7, and later (for developers) Android - ARM processors ##### ##### Installation Software The usb2isa software includes UNIVERSAL SOFTWARE LAYER feature. We currently offer support for DOS under Widows operating systems. Pre-order Considerations 1. Powering needs. We have a number of power supplies which can provide +5V, -5V, +12V, and -12V for the ISA cards mounted on the USB2ISA-R product. To find whether you need a Power Supply, please read ISA card - finding the voltages used. 2. Enclosures. ARS Technologies provides plastic enclosures/boxes for mounting of USB2ISA-R and 1 ISA card. Please check the dimensions on the enclosures and cards before ordering - ISA-PCI-B1 or ISA-PCI-B2, to ensure that the box will fit your ISA card. 3. Cables. The USB2ISA-R product and the computer system connect with a cable. You can use one of the choices of cables we offer – 3 feet or 15 feet. 4. Software. The installation software should provide all the software you would need to get our USB2ISA-R card to work with your ISA card. We offer our SDKBUS product for developers. If you have access to the ISA software source code, you may be interested in our SDKBUS. Price - in US Dollars: $149US each ARS Technologies offers quantity discounts as follows: 5-19 units, $144 each 20-100 units, $139 each 100+ units, please ask for a quote
Use the form below to email a friend about this product. Required fields are marked with a star (*). Click the 'Submit' button at the bottom of this form to proceed. Email Addresses
Your Email Address* Your Email Address* Enter your email address. | Your Friend's Address* Your Friend's Address* Enter your friend's email address.
Message
Message* Message* Enter a message to include with the product information.
| Quick Store Search Search Term Advanced Search Currencies Select Currency Account Menu Account Login Create New Account Delivery Address Book Email Subscriptions Send Contact Message Recently Visited Pages sdkbus2 - SDK 2.0 for USB2 and SSI2 products sdkbus2 - SDK 2.0 for USB2 and SSI2 products isa-pci-b2 - Enclosure Dbl. length for 1 ISA/PCI/PCIe card isa-pci-b2 - Enclosure Dbl. length for 1 ISA/PCI/PCIe card isa-pci-b1 - Enclosure for 1 ISA/PCI/PCIe card Popular Pages ARS Technologies Inc. Shopping Cart Send Contact Message USB 2.0 XPRS

Software: ClickCartPro, Copyright 1999-2024 Kryptronic, Inc. Exec Time: 0.291762 Seconds Memory Usage: 4.019691 Megabytes