| Login to enhance your online experience. Login or Create an Account
Categories USB 2.0 XPRS Power Supplies Enclosures Cables Software Main Menu About Us Knowledge-Base FAQS Blog Installation Software Technical-Support News Mail-List Store-Policies License-Agreement Terms-Of -Use Privacy-Statement Online Store Menu Store Home Shopping Cart Checkout Advanced Search Shopping Cart There are no items in your shopping cart. | # Assembly Instructions For The ISA-PCI-B2 [Click on images to enlarge] Step 1: Place 4 screws in the plastic shell with 4 holes. Step 2: Place the usb2isa / ssi2-isa card holes for attaching in the screws and fasten with nuts. Step 3: Plug the ISA card in the slot of the usb2isa / ssi2-isa card. Step 4: Place the cover of the box - depending on the height of the ISA card, and fix the cover with 4 screws to the shell. Fix the metal bracket of the ISA card to the cover - directly or with the plastic spacer. Step 5: The usb2isa / ssi2-isa and the ISA cards are ready for use - place in a horizontal or vertical position as desired. | Quick Store Search Search Term Advanced Search Currencies Select Currency Account Menu Account Login Create New Account Delivery Address Book Email Subscriptions Send Contact Message Recently Visited Pages Assembly of ISA-PCI-B2 Assembly of ISA-PCI-B1 Assembly of ISA-PCI-B1 usb2isa-r - USB 2.0 to ISA card ROHS usb2isa-r - USB 2.0 to ISA card ROHS Popular Pages ARS Technologies Inc. Shopping Cart Send Contact Message USB 2.0 XPRS

Software: ClickCartPro, Copyright 1999-2024 Kryptronic, Inc. Exec Time: 0.274961 Seconds Memory Usage: 3.62925 Megabytes