| Login to enhance your online experience. Login or Create an Account
Categories USB 2.0 XPRS Power Supplies Enclosures Cables Software Main Menu About Us Knowledge-Base FAQS Blog Installation Software Technical-Support News Mail-List Store-Policies License-Agreement Terms-Of -Use Privacy-Statement Online Store Menu Store Home Shopping Cart Checkout Advanced Search Shopping Cart There are no items in your shopping cart. | # Assembly Instructions For The ISA-X3-B1 [Click on images to enlarge] . Step 1: Place 4 screws in the plastic shell with 4 holes. Step 2: Place the usb2isa-x3 / ssi2-isa-x3 card holes for attaching in the screws and fasten with nuts. Step 3: Plug the ISA cards in the slot of the usb2isa-x3 / ssi2-isa-x3 card. Step 4: Place the cover of the box - depending on the height of the ISA cards, and fix the cover with 4 screws to the shell. Fix the metal brackets of the ISA cards to the cover - directly or with the plastic spacers. Step 5: The usb2isa-x3 / ssi2-isa-x3 and the ISA cards are ready for use - place in a horizontal or vertical position as desired. | Quick Store Search Search Term Advanced Search Currencies Select Currency Account Menu Account Login Create New Account Delivery Address Book Email Subscriptions Send Contact Message Recently Visited Pages Assembly-ISA-X3-b1 Assembly of ISA-PCI-B2 Assembly of ISA-PCI-B2 Assembly of ISA-PCI-B1 Assembly of ISA-PCI-B1 Popular Pages ARS Technologies Inc. Shopping Cart Send Contact Message USB 2.0 XPRS

Software: ClickCartPro, Copyright 1999-2024 Kryptronic, Inc. Exec Time: 0.271805 Seconds Memory Usage: 3.629257 Megabytes