| Login to enhance your online experience. Login or Create an Account
Categories USB 2.0 XPRS Power Supplies Enclosures Cables Software Main Menu About Us Knowledge-Base FAQS Blog Installation Software Technical-Support News Mail-List Store-Policies License-Agreement Terms-Of -Use Privacy-Statement Online Store Menu Store Home Shopping Cart Checkout Advanced Search Shopping Cart There are no items in your shopping cart. | # Email a Friend Menu: Store Home | Advanced Search | Shopping Cart | Checkout
xprs-cpcie - XPRS Compact PCI Express card [Click on image to enlarge] Tweet The XPRS-cPCIe connects with one of our XRPS-HOST-.. cards, and allows using of Compact PCI Express, or PXI Express type card outside of a computer system. ROHS compliant - Yes, recommended for customers in the European Union, and all other countries. ### Installing and use of XPRS-cPCIe - click for details and images. If you have a Compact PCI Express or PXI Express type peripheral card, you can use it outside of this computer system: - PCI Express desktop, with our xprs-host-dt product - ExpressCard notebook, with our xprs-host-ec product Software support The XPRS line of products function on all operating systems which have support for PCI Express (desktop), or ExpressCard (notebook) systems. Our installation software offers additional software support under: - Windows - 2000, XP, Server 2003, Vista, Server 2008, 7, 8.1 - Linux - 3.x.xx kernels - Mac OS X 10.5, and later Pre-order Considerations 1. Choose a host card. The xprs-cpcie is supported by a variety of host cards. A selection for choosing of a host card is included on this ordering page: - xprs-host-dt on a PCI Express desktop system - or, xprs-host-ec on a notebook system with an ExpressCard slot Or, you can order separately host cards on their product pages. 2. Powering needs and Enclosures. The Compact PCI Express, or PXI Express interface requires either 3.3V only, or 3.3V and 12V to be supplied for the cPCIe / PXIe card. If a peripheral card uses 3.3V only with low current consumption, the card may be powered directly through the cables. If unsure on the power requirements of a particular cPCIe / PXIe card, please use our PWR-3V products to have 3.3V power supplied to XPRS-cPCIe for the cPCIe / PXIe card. 3. Software developers. The installation software includes a simple / basic API set for software developers. Our SDKBUS product has an extensive API set for software developers as well. If you have access to the source code for the specific peripheral card, and want to have it supported under Windows, Linux, Mac OS X, you may consider using our API set. Price - in US Dollars: $89US each ARS Technologies offers quantity discounts as follows: 5-19 units, $85 each 20-100 units, $82 each 100+ units, please ask for a quote
Use the form below to email a friend about this product. Required fields are marked with a star (*). Click the 'Submit' button at the bottom of this form to proceed. Email Addresses
Your Email Address* Your Email Address* Enter your email address. | Your Friend's Address* Your Friend's Address* Enter your friend's email address.
Message
Message* Message* Enter a message to include with the product information.
| Quick Store Search Search Term Advanced Search Currencies Select Currency Account Menu Account Login Create New Account Delivery Address Book Email Subscriptions Send Contact Message Recently Visited Pages pwr-3v - External Power Supply 3.3V pwr-3v - External Power Supply 3.3V Installing and use of XPRS-HOST-EC Installing and use of XPRS-cPCIe Installing and use of XPRS-HOST-EC Popular Pages ARS Technologies Inc. Shopping Cart Send Contact Message USB 2.0 XPRS

Software: ClickCartPro, Copyright 1999-2024 Kryptronic, Inc. Exec Time: 0.180484 Seconds Memory Usage: 4.019241 Megabytes