| Login to enhance your online experience. Login or Create an Account
Categories USB 2.0 XPRS Power Supplies Enclosures Cables Software Main Menu About Us Knowledge-Base FAQS Blog Installation Software Technical-Support News Mail-List Store-Policies License-Agreement Terms-Of -Use Privacy-Statement Online Store Menu Store Home Shopping Cart Checkout Advanced Search Shopping Cart There are no items in your shopping cart. | [Click images to enlarge] The ARS Technologies power supply module is designed for the USB2ISA, USB2ISA-X3 SSI2-ISA, SSI2-ISA-X3, SSI2-PCI, SSI2-PCI-X3 XPRS-PCI, XPRS-PCI-X3 Dimensions: 0.5 X 0.25 X 0.3 inches. The power supply module provides additional voltages as follows: -5V/100mA +12V/45mA -12V/45mA for the ISA card(s). The power supply module is powered through USB cable, so there is no need of external cables or an external power supply when using the isa-pwr. To find the voltages of the peripheral card and do you need the Power Supply Module, please read these articles: - for ISA cards . - for PCI cards . INSTALLING THE POWER SUPPLY MODULE (ISA-PWR) [Click on images to enlarge] # How To Install The POWER SUPPLY MODULE The POWER SUPPLY MODULE (ISA-PWR) can be installed on the USB2ISA USB2ISA-X3 or Installing the POWER SUPPLY MODULE IS SIMPLE. Step 1 Place the POWER SUPPLY MODULE on a flat surface so that the five silver pins of the POWER SUPPLY MODULE are closest to the surface. Step 2 Pick up the isa-pwr and insert the five silver pins into the 6-pin connector that is next to the ISA slot on the USA2ISA, USB2ISA-X3, card. NOTE 1: On of the connectors in the 6-pin connector will remain empty because the isa-pwr only has five pins. Look at the images below for a visual demonstration of installing the isa-pwr (POWER SUPPLY MODULE) Theses instructions are the same for installing the isa-pwr on the USB2ISA, USB2ISA-X3. NOTE 2: When applying the isa-pwr, please make sure to change your jumper settings as explained in the User’s Guide. The USB2ISA-RA are shown below. The POWER SUPPLY MODULE is placed as it would be before the isa-pwr is attached to the USB2ISA . ## The USB2ISA before the ISA-PWR is attached. | The isa-pwr is aligned with the 6-pin connector on the USB2ISA .

## Installing the ISA-PWR on the USB2ISA

| Step 1: Position the isa-pwr so that it is aligned with the 6-pin header on the USB2ISA. The 6-pin header is next to the ISA slot on the USB2ISA.
| Step 2: Place the isa-pwr into the 6-pin connector and gently press down.

Quick Store Search

Search Term

Advanced Search
Currencies

Select Currency

Account Menu

- Account Login
- Create New Account
- Delivery Address Book
- Email Subscriptions
- Send Contact Message

Recently Visited Pages

- SDKBUS-VS-USL
- Power-Supply-Mod-Install
- SDKBUS-VS-USL
- LINUX-SUPPORT
- LINUX-SUPPORT

Popular Pages

- ARS Technologies Inc.
- Shopping Cart
- Send Contact Message
- USB 2.0
- XPRS

Software: ClickCartPro, Copyright 1999-2024 Kryptronic, Inc. Exec Time: 0.234798 Seconds Memory Usage: 3.632172 Megabytes