| Login to enhance your online experience. Login or Create an Account
Categories USB 2.0 XPRS Power Supplies Enclosures Cables Software Main Menu About Us Knowledge-Base FAQS Blog Installation Software Technical-Support News Mail-List Store-Policies License-Agreement Terms-Of -Use Privacy-Statement Online Store Menu Store Home Shopping Cart Checkout Advanced Search Shopping Cart There are no items in your shopping cart. | Tweet # Installing and use of XPRS-HOST-DT ## 1. Introduction The XPRS-HOST-DT is mounted in a desktop computer system with PCI Express slots. [Click to enlarge] The kit of XPRS-HOST-DT product includes a metal bracket and 2 cables with length of 1.6ft / 0.5m. ## 2. Assembly of XPRS-HOST-DT A desktop computer system with PCI Express slots normally includes 1 x16 PCI Express slot - shown on upper side, and one or more x1 PCI Express slots - 2 slots on this image. [Click to enlarge] The image below shows - mounted XPRS-HOST-DT in one PCI Express x1 slot, and mounted and attached metal bracket. [Click to enlarge] Put the cables through the opening of the bracket. To assist with the mounting of cables, remove XPRS-HOST-DT, connect cables, and place again in the same PCI Express x1 slot. [Click to enlarge] The XPRS-HOST-DT allows multiple ways of use - as shown below. ## 3. Additional ways of use ### 3.1. Using xprs-host-dt in a PCI Express x16 slot The PCI Express standard has compatibility between x1, x4, x8, x18 interfaces. [Click to enlarge] The XPRS-HOST-DT allows plugging in a PCI Express x16 slot and using it from there. ### 3.2. Using multiple xprs-host-dt cards A desktop computer system with PCI Express slots normally includes multiple PCI Express slots. [Click to enlarge] Multiple XPRS-HOST-DT cards may be mounted in the desktop system - up to the total number of available PCI Express x16 slots. ### 3.3. Extending length The XPRS-HOST-DT kit includes 2 cables with length of 1.6ft / 0.5m. [Click to enlarge] We offer 3ft / 1m cables set - to extend the length. Please note that the cables carry 3.3V which can power the mounted on the other side of the cable peripheral card. Using longer cable may reduce the total current available for the mounted peripheral card. ## 4. Next step The next step is installing of XPRS-.. card together with a peripheral card: - xprs-px-x1 with a PCI Express X1 card - xprs-px-x16 with a PCI Express X16 card - xprs-pci-x1 with a PCI card - xprs-cb with a PCMCIA CardBus card - xprs-ec with an ExpressCard card | Quick Store Search Search Term Advanced Search Currencies Select Currency Account Menu Account Login Create New Account Delivery Address Book Email Subscriptions Send Contact Message Recently Visited Pages Installing and use of XPRS-HOST-DT Installing and use of XPRS-CB Installing and use of XPRS-CB Installing and use of XPRS-PCI-X1 Installing and use of XPRS-PCI-X1 Popular Pages ARS Technologies Inc. Shopping Cart Send Contact Message USB 2.0 XPRS

Software: ClickCartPro, Copyright 1999-2024 Kryptronic, Inc. Exec Time: 0.167512 Seconds Memory Usage: 3.633751 Megabytes