| Login to enhance your online experience. Login or Create an Account
Categories USB 2.0 XPRS Power Supplies Enclosures Cables Software Main Menu About Us Knowledge-Base FAQS Blog Installation Software Technical-Support News Mail-List Store-Policies License-Agreement Terms-Of -Use Privacy-Statement Online Store Menu Store Home Shopping Cart Checkout Advanced Search Shopping Cart There are no items in your shopping cart. | # Speed testing -x16 vs. -x1 with PCI Express video cards ## 1. Introduction Our xprs-px-x16 product allows using of PCI Express -x16 cards, outside of computer systems through cables. For details on the way of use, you can check this article . Number of our customers, interested in using this product, asked technical details. The xprs-px-x16 allows using of a PCI Express -x16 card, through -x1 link and cables. In general, one -x16 card, has 16 transmit and 16 receive pairs/lines. One -x1 card, has 1 transmit and 1 receive pair/line. Theoretically a -x16 card has to be 16 times faster than one -x1 card. PCI Express interface allows the work of a card, using the smaller number of transmit/receive pairs. This article compares the speed difference when the same -x16 card works using all 16 transmit/receive pairs, and when the card works using 1 transmit/receive pair. ## 2. Way of testing PCI Express -x16 card normally is mounted on a desktop motherboard. ##### (click on image to enlarge) The above image is a very simplified representation of mounting. A desktop motherboard is normally mounted in a box, hooked to a power supply ... etc. The image below shows the same video card mounted on our xprs-px-x16 product, connected through 1m cables, to xprs-host-dt mounted on the same motherboard. The above image is a also simplified representation of mounting. The xprs-px-x16 product has to be connected to a power supply in order to power on the PCI Express -x16 card. ## 3. Cards and tests The tests wre performed on 2 video cards, both of them based on NVIDIA chips: - geforce 8400 card, 512mb memory (card on right side) - geforce GT 430 card, 1gb memory (card on left side) As a result of a web search for doing a benchmark test on a video card, we picked 2 tests: - by Freestone-Group - free download by Passmark Software - 30 days free for evaluation, cost The Freestone-Group test software (image above) is only for benchmarking video cards and gives a single score as the end result. The Passmark test software (image below) is for general benchmarking of a system, includes 2D and 3D tests for video cards, and gives separate scores for the each of the sub-tests. ## 4. Test results The Freestone-Group test gives these scores:
     Card        -x16        -x1     Difference
    '8400'        44          40      9%
    'gt 430'      238         231     2.9%
The Freestone-Group mix of tests like the above show a very small difference between -x16 and -x1 mode. The Passmark test gives these scores for '8400' card:
       Test                           -x16    -x1    Difference
    Graphics 2D - Solid Vectors:       0.9     0.9    0
    Graphics 2D - Transparent Vectors: 0.9     0.8   11.1%
    Graphics 2D - Complex Vectors:     87.1   84.1    3.4%
    Graphics 2D - Fonts and Text:      36.3   28.8   20.6$
    Graphics 2D - Windows Interface:   14.0   11.2   20.0%
    Graphics 2D - Image Filters:       92.3   88.4    4.2%
    Graphics 2D - Image Rendering:    202.2  141.5   30.0%
    Graphics 3D - Simple:             130.5   83.1   36.3%
    Graphics 3D - Medium:              50.6   34.4   32.0%
    Graphics 3D - Complex:             14.7    2.3   84.3% !!!
    Graphics 3D - DirectX 10:           0.9    0.9    0
    2D Graphics Mark:                 157.7  135.7   13.9%
    3D Graphics Mark:                 117.9   65.7   42.2%
The Passmark test gives these scores for 'gt 430' card:
       Test                              -x16     -x1    Difference
    Graphics 2D - Solid Vectors:          1.0     1.0    0
    Graphics 2D - Transparent Vectors:    1.0     1.0    0
    Graphics 2D - Complex Vectors:       91.4    77.4   15.3%
    Graphics 2D - Fonts and Text:        36.1    35.5    1.6%
    Graphics 2D - Windows Interface:     14.0    14.0    0
    Graphics 2D - Image Filters:         92.6    92.4   0.1%
    Graphics 2D - Image Rendering:      203.7   203.1   0.3%
    Graphics 3D - Simple:               406.5   396.9   2.3%
    Graphics 3D - Medium:               271.3   204.5  24.6%
    Graphics 3D - Complex:               16.0     4.0  75.0% !!!
    Graphics 3D - DirectX 10:             7.4     4.9  33.7%
    2D Graphics Mark:                   162.1   156.0   3.7%
    3D Graphics Mark:                   460.0   337.5  26.6%
The tests show a very small difference for the 2D Graphics tests. A large difference appears for the Complex 3D Graphics test. However the larger the video memory is and the better/faster the GPU - the gap between -x16 and -x1 modes gets smaller. Conclusion - a PCI Express -x16 card placed in '-x1' mode is getting most of the performance, and may be good enough solution in case of using a peripheral card outside of a computer system, through a cable. ## 5. DIY (do-it-yourself) testing While we did test with 2 video cards, they are most likely different your own video card(s). If you are curious about what the difference is between -x16 and -x1 modes for your video cards, there is a way to find this. The PCI Express connectors have compatible pin-outs - with the signals on the pins on the -x1 connector identical to the respective pins for the part of the -x16 connector. In practice this means that you can plug one -x1 card into a -x16 connector an it will still work. The opposite is also true - using a tape, you can cover the additional pins of one -x16 card, and leave exposed only pins matching -x1 connector. When you plug a -x16 video card prepared in such way in a motherboard, it will be forced to operate in -x1 mode. Then you can run some of the above tests or any other test you like. After testing, when the tape is removed, please make sure the pins on the -x16 card are cleaned with alcohol or other solutions. | Quick Store Search Search Term Advanced Search Currencies Select Currency Account Menu Account Login Create New Account Delivery Address Book Email Subscriptions Send Contact Message Recently Visited Pages Speed testing -x16 vs. -x1 with PCI Express video cards Linux driver - binary builder kit (BBK) Linux driver - binary builder kit (BBK) Image maker tool -img-mk Image maker tool -img-mk Popular Pages ARS Technologies Inc. Shopping Cart Send Contact Message USB 2.0 XPRS

Software: ClickCartPro, Copyright 1999-2024 Kryptronic, Inc. Exec Time: 0.192751 Seconds Memory Usage: 3.636429 Megabytes