| Login to enhance your online experience. Login or Create an Account
Categories USB 2.0 XPRS Power Supplies Enclosures Cables Software Main Menu About Us Knowledge-Base FAQS Blog Installation Software Technical-Support News Mail-List Store-Policies License-Agreement Terms-Of -Use Privacy-Statement Online Store Menu Store Home Shopping Cart Checkout Advanced Search Shopping Cart There are no items in your shopping cart. | # xprs-pci-x3 - XPRS PCI 3 connectors card Menu: Store Home | Advanced Search | Shopping Cart | Checkout Location: Store Home > XPRS > xprs-pci-x3 - XPRS PCI 3 connectors card
xprs-pci-x3 - XPRS PCI 3 connectors card [Click on image to enlarge] Tweet The XPRS-PCI-X3 connects with one of our XRPS-HOST-.. cards, and allows using of up to 3 PCI type cards outside of a computer system. ROHS compliant - Yes, recommended for customers in the European Union, and all other countries. ### Installing and use of XPRS-PCI-X3 - click for details and images. If you have PCI type peripheral cards, you can use them outside of this computer system: - PCI Express desktop, with our xprs-host-dt product - ExpressCard notebook, with our xprs-host-ec product Software support The XPRS line of products function on all operating systems which have support for PCI Express (desktop), or ExpressCard (notebook) systems. Our installation software offers additional software support under: - Windows - 2000, XP, Server 2003, Vista, Server 2008, 7, 8.1, 10 - Linux - 3.x.xx and later kernels - Mac OS X 10.5, and later Pre-order Considerations 1. Choose a host card. The xprs-pci-x3 is supported by a variety of host cards. A selection for choosing of a host card is included on this ordering page: - xprs-host-dt on a PCI Express desktop system - or, xprs-host-ec on a notebook system with an ExpressCard slot Or, you can order separately host cards on their product pages. 2. Powering needs and Enclosures. The PCI interface requires either 3.3V, or 5V, or both voltages to be supplied for the PCI card. PCI cards may optionally use also +12V and -12V for powering. To find whether you need a Power Supply, please read - PCI card - finding the voltages used. If a peripheral card only uses 3.3V / 5V you can use one of our PWR-5V products to have 3.3V / 5V power supplied to XPRS-PCI-X1 for the PCI card. If a PCI peripheral card needs +12V and -12V with current consumption of up to 50mA, you can add to PWR-5V the power module . If a PCI peripheral card needs +12V and -12V with high current consumption, or if unsure on the power requirements of a particular PCI card, you can use the ISA-PWR-XR external power supply. The XPRS-PCI-X3 together with the PCI type cards may be mounted in an enclosure. Small PCI type cards may be put in ISA-X3-B1 enclosure. Longer and larger PCI type cards may be put in our ISA-X3-B2 enclosure. 3. Software developers. The installation software includes a simple / basic API set for software developers. Our SDKBUS product has an extensive API set for software developers as well. If you have access to the source code for the specific peripheral card, and want to have it supported under Windows, Linux, Mac OS X, you may consider using our API set.
Google Site Stats - send feedback
Price - in US Dollars: $149US each ARS Technologies offers quantity discounts as follows: 5-19 units, $145 each 20-100 units, $142 each 100+ units, please ask for a quote This item is currently out of stock. Email This Item to a Friend
| Quick Store Search Search Term Advanced Search Currencies Select Currency Account Menu Account Login Create New Account Delivery Address Book Email Subscriptions Send Contact Message Recently Visited Pages xprs-pci-x3 - XPRS PCI 3 connectors card xprs-pci-x1 - XPRS PCI peripheral card xprs-pci-x1 - XPRS PCI peripheral card XPRS XPRS Popular Pages ARS Technologies Inc. Shopping Cart Send Contact Message USB 2.0 XPRS

Software: ClickCartPro, Copyright 1999-2024 Kryptronic, Inc. Exec Time: 0.319939 Seconds Memory Usage: 3.986954 Megabytes