| Login to enhance your online experience. Login or Create an Account
Categories USB 2.0 XPRS Power Supplies Enclosures Cables Software Main Menu About Us Knowledge-Base FAQS Blog Installation Software Technical-Support News Mail-List Store-Policies License-Agreement Terms-Of -Use Privacy-Statement Online Store Menu Store Home Shopping Cart Checkout Advanced Search Shopping Cart There are no items in your shopping cart. | Tweet # Installing and use of XPRS-EC ## 1. Introduction The XPRS-EC connects with one of our XRPS-HOST-.. cards, and allows using of ExpressCard type34 and type54 peripheral cards outside of a computer system. [Click to enlarge] The image shows XPRS-EC product, cables coming from XRPS-HOST-.. card, and one ExpressCard type34 peripheral card. ExpressCard type54 peripheral card is supported as well. ## 2. Preliminary step Based on the computer system one preliminary step is installing of a XPRS-HOST-.. card: - xprs-host-dt on a PCI Express desktop system - or, xprs-host-ec on a notebook system with an ExpressCard slot ## 3. Assembly of XPRS-EC There are 2 ways to connect the 2 cables to the connectors on XPRS-EC. [Click to enlarge] Make sure that the XPRS-HOST-.. card is inserted, and the host computer system is powered on. The image above shows the wrong way of connecting the cables to the connectors - the onboard LED is not lit, the LED is not on. In such case remove both cables, switch positions, and plug to the other connectors. The image below shows the right way - the onboard LED is lit, the LED is on. [Click to enlarge] ## 4. Insert / remove of peripheral cards When the host system is a notebook, and the operating system supports ExpressCard slots, you can dynamically insert/remove ExpressCard type34 or type54 card on XPRS-EC. When the host system is a desktop, or the operating system does not support hot insert/ remove of PCI Express based peripherals you need to: - power off host system - mount XPRS-HOST-.. in the system - connect cables to XPRS-EC - in the proper way - mount ExpressCard type34 or type54 card - power on host system [Click to enlarge] ARSTech Enumerator provides indication of events, and additional software support for hot insert / remove. | Quick Store Search Search Term Advanced Search Currencies Select Currency Account Menu Account Login Create New Account Delivery Address Book Email Subscriptions Send Contact Message Recently Visited Pages Installing and use of XPRS-EC Installing and use of XPRS-cPCIe Installing and use of XPRS-cPCIe Installing and use of XPRS-EC Installing and use of XPRS-EC Popular Pages ARS Technologies Inc. Shopping Cart Send Contact Message USB 2.0 XPRS

Software: ClickCartPro, Copyright 1999-2024 Kryptronic, Inc. Exec Time: 0.451595 Seconds Memory Usage: 3.632408 Megabytes